{"text_format":"3","workbook":"xls","n_sheets":7,"sheets":["超凡","01","50","生化360","15","索诺声","PLDD"],"not_rendered":{"images":2,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"超凡","index":0,"n_rows":34,"n_cols":10,"rows_kept":34,"merged":[[0,0,0,3],[1,0,1,9],[2,0,2,9],[3,0,3,9],[4,0,26,0],[4,1,4,9],[5,1,5,9],[6,1,6,9],[7,1,7,9],[8,1,8,9],[9,1,9,9],[10,1,10,9],[11,1,11,9],[12,1,12,9],[13,1,13,9],[14,1,14,9],[15,1,15,9],[16,1,16,9],[17,1,17,9],[18,1,18,9],[19,1,19,9],[20,1,20,9],[21,1,21,9],[22,1,22,9],[23,1,23,9],[24,1,24,9],[25,1,25,9],[26,1,26,9],[27,0,29,0],[27,1,27,9],[28,1,28,9],[29,1,29,9],[30,0,30,9],[31,0,31,9],[32,0,32,1],[32,2,32,3],[32,4,32,5],[32,6,32,8],[33,0,33,1],[33,2,33,3],[33,4,33,5],[33,6,33,8]],"flags":["formulas_cached_only"]}
["附件1："]
["捐助设备清单"]
[]
["原装飞利浦超凡影像(升级版)彩超"]
["标准配置 ","超凡影像升级版-主机"]
[null,"中文操作系统"]
[null,"全数字512通道"]
[null,"宽频声束形成器"]
[null,"飞利浦专利的融合成像技术"]
[null,"主机频带1-15MHZ"]
[null,"组织谐波成像应用于腹部、小器官、心脏探头"]
[null,"高敏感彩色多普勒"]
[null,"能量图/方向能量图"]
[null,"脉冲多普勒/三实时，连续多普勒"]
[null,"彩色M型成像"]
[null,"彩色对比成像"]
[null,"梯形成像(线阵探头)"]
[null,"侧向增益补偿功能"]
[null,"高分辨率放大功能"]
[null,"自由臂三维成像"]
[null,"图文报告的编辑(可插入图像)"]
[null,"内置的图像数据管理"]
[null,"动、静态图像可硬盘存储、光盘刻录态"]
[null,"心脏、全身应用软件及测量、计算软件"]
[null,"中文操作手册"]
[null,"维修手册"]
[null,"17″真彩无间隔显示器"]
["探头配置","S4-2 心脏相控阵探头"]
[null,"C5-2 腹部凸阵探头"]
[null,"L12-3 38MM线阵探头"]
["上述产品标准配置报价为110万人民币"]
[]
["产品名称",null,"报   价",null,"招  标  价",null,"国家中医局补贴",null,null,"医院实付金额"]
["原装飞利浦超凡影像彩色多普勒超声诊断系统 (升级版)                 ",null,"110万人民币",null,"58万人民币",null,"20万人民币",null,null,"38万人民币"]

{"sheet":"01","index":1,"n_rows":47,"n_cols":9,"rows_kept":47,"merged":[[0,0,0,10],[1,0,1,10],[3,0,34,0],[3,1,3,10],[4,1,4,10],[5,1,5,10],[6,1,6,10],[7,1,7,10],[8,1,8,10],[9,1,9,10],[10,1,10,10],[11,1,11,10],[12,1,12,10],[13,1,13,10],[14,1,14,10],[15,1,15,10],[16,1,16,10],[17,1,17,10],[18,1,18,10],[19,1,19,10],[20,1,20,10],[21,1,21,10],[22,1,22,10],[23,1,23,10],[24,1,24,10],[25,1,25,10],[26,1,26,10],[27,1,27,10],[28,1,28,10],[29,1,29,10],[30,1,30,10],[31,1,31,10],[32,1,32,10],[33,1,33,10],[34,1,34,10],[35,1,35,10],[36,1,36,10],[37,0,39,0],[37,1,37,10],[38,1,38,10],[39,1,39,10],[41,1,41,10],[42,0,42,10],[43,1,43,5],[44,3,44,4],[44,5,44,7],[44,8,44,10],[45,3,45,4],[45,5,45,7],[45,8,45,10],[46,3,46,4],[46,5,46,7],[46,8,46,10]],"flags":["formulas_cached_only"]}
["    ULTRASONIX"]
["原装进口加拿大ES01彩超标准版配置清单"]
[]
["系统标准配置","多种语言操作界面"]
[null,"高清自动优化成像"]
[null,"超宽频带数字化声束形成器"]
[null,"512~1024数字化通道"]
[null,"170dB动态范围"]
[null,"二维、M型成像"]
[null,"彩色多普勒,脉冲多普勒,连续多普勒"]
[null,"彩色能量血管造影(能量图)"]
[null,"组织谐波成像"]
[null,"梯形成像"]
[null,"宽视野成像"]
[null,"自由臂三维成像"]
[null,"一体化图像管理"]
[null,"InterNet联网"]
[null,"DICOM3.0支持"]
[null,"电子邮件支持"]
[null," CD/DVD 刻录"]
[null,"全自动病人优选设置"]
[null,"2D,脉冲及彩色多普勒三同步"]
[null,"电影回放, M型及多普勒回放"]
[null,"产科,血管,心脏,前列腺,妇科分析软件包"]
[null,"高分辨率放大"]
[null,"伪彩色"]
[null,"可选择回放格式"]
[null,"测量工具包括: 直线距离,面积,周长, 容积"]
[null,"自动多普勒分析"]
[null,"使用者自设定测量"]
[null,"快速自动注释"]
[null,"快速用户自定义设置"]
[null,"17寸高分辨率彩色液晶显示器"]
[null,"在线帮助功能"]
[null,"通过光盘或因特网智能软件升级"]
["临床软件包","全身临床软件包（包括腹部、血管、乳腺、产科、小儿科/新生儿、心脏、前列腺、妇产科、骨骼肌肉）"]
["操作手册","中文"]
["探头标准配置","PA4-2超宽频带相控阵"]
[null,"C5-2超宽频带凸阵"]
[null,"L14-5 38mm超宽频带线阵"]
["选配功能","实时4D软件 "]
["选配探头","4DC6-3容积三维超宽频带凸阵"]
["上述产品标准配置报价为160万人民币"]
[]
["产品名称","报  价","招标价","阳光工程补额度",null,"国家中医局补贴",null,null,"医院实付金额"]
["原装加拿大全数字化彩色多普勒超声诊断系统                  Ultrasonix ES01(标准版配置)","160万人民币","59.8万人民币","10万人民币",null,"20万人民币",null,null,"29.8万人民币"]
["选配4D探头及功能",null,"20万人民币","10万人民币",{"$nulls":4},"10万人民币"]

{"sheet":"50","index":2,"n_rows":46,"n_cols":10,"rows_kept":46,"merged":[[0,0,0,9],[1,0,1,9],[3,1,3,9],[4,1,4,9],[5,1,5,9],[6,1,6,9],[7,1,7,9],[8,1,8,9],[9,1,9,9],[10,1,10,9],[11,1,11,9],[12,1,12,9],[13,1,13,9],[14,1,14,9],[15,1,15,9],[16,1,16,9],[17,1,17,9],[18,1,18,9],[19,1,19,9],[20,1,20,9],[21,1,21,9],[22,1,22,9],[23,1,23,9],[24,1,24,9],[25,1,25,9],[26,1,26,9],[27,1,27,9],[28,1,28,9],[29,1,29,9],[30,1,30,9],[31,1,31,9],[32,1,32,9],[33,1,33,9],[34,1,34,9],[35,1,35,9],[36,1,36,9],[37,1,37,9],[38,1,38,9],[39,1,39,9],[40,1,40,9],[41,1,41,9],[42,0,42,9],[43,3,43,6],[44,0,44,1],[44,2,44,3],[44,4,44,5],[44,7,44,8],[45,0,45,1],[45,2,45,3],[45,4,45,5],[45,7,45,8]],"flags":["formulas_cached_only"]}
["   ESAOTE"]
["原装进口意大利百胜My LabTM50彩超配置清单(SUN)"]
[]
["系统基本配置","MyLab50 100-240V/50-60HZ 彩色超声系统"]
[null,"多功能、多用途全数字主机,包括17英寸高分辩率S-VGA彩色监视器。通过可选许可证升级。"]
[null,"选择可选件获得DICOM全功能。"]
[null,"应用："]
[null,"全身应用"]
[null,"发射："]
[null,"探头具有独立数字延迟，可变多点聚集功能"]
[null,"接收："]
[null,"数字波束形成完成二维成像、彩色和多普勒功能。可变孔径和动态聚焦。"]
[null,"常规包括："]
[null,"双处理器。UNIX和Windows XP操作系统。"]
[null,"高敏感性CFM和能量多普勒"]
[null,"PW，HPRF和可变角CW功能"]
[null,"静态和动态图象PC格式兼容存储（BMP，AVI）"]
[null,"四探头连接方式（三电子探头接口和一个多普勒探头接口）"]
[null,"实时档案存储功能（Real Time Archive)"]
[null,"CD刻录"]
[null,"内部硬盘存储"]
[null,"USB优盘存储"]
[null,"S-VGA，RGB，S-VHS，复合视频信号输出"]
[null,"NTSC/PAL视频格式"]
[null,"多语言软件系统，通过CD未来升级功能"]
[null,"根据选择的许可证，获得各种测量软件"]
[null,"在线和离线常规测量功能"]
[null,"EN 60601-1，EN 60601-1-2,EN 30993-1,EN 61157安全标准"]
[null,"系统同时还包括："]
[null,"用户操作手册"]
[null,"欧洲标准电源联线"]
[null,"彩色成像模块"]
[null,"多普勒模块"]
[null,"TEI组织谐波驱动许可"]
[null,"解剖M超"]
[null,"常规成像（腹部、甲状腺、肌肉骨骼、乳腺、心脏、小器官等）"]
[null,"动态图象存储功能"]
[null,"线阵和高频成像模块"]
[null,"凸阵和相控阵成像模块"]
["探头标准配置","CA421  40R电子凸阵探头(腹部探头)"]
[null,"LA523E 电子线阵探头(小器官探头)"]
[null,"PA230E　电子相控阵探头(心脏探头)"]
["上述产品标准配置报价为230万人民币"]
[]
["产品名称",null,"报   价",null,"招 标 价",null,"阳光工程补额度","国家中医局补贴",null,"医院实付金额"]
["原装意大利百胜彩色多普勒超声诊断系统  My LabTM 50        ",null,"230万人民币",null,"98万人民币",null,"20万人民币","20万人民币",null,"58万人民币"]

{"sheet":"生化360","index":3,"n_rows":30,"n_cols":10,"rows_kept":30,"merged":[[0,0,1,9],[2,0,2,9],[3,0,3,9],[4,1,4,9],[5,1,5,9],[6,1,6,9],[7,1,7,9],[8,1,8,9],[9,1,9,9],[10,1,10,9],[11,1,11,9],[12,1,12,9],[13,1,13,9],[14,1,14,9],[15,1,15,9],[16,1,16,9],[17,1,17,9],[18,1,18,9],[19,1,19,9],[20,1,20,9],[21,1,21,9],[22,1,22,9],[23,1,23,9],[24,1,24,9],[25,1,25,9],[26,0,26,9],[28,0,28,1],[28,2,28,3],[28,4,28,5],[28,6,28,8],[29,0,29,1],[29,2,29,3],[29,4,29,5],[29,6,29,8]],"flags":["formulas_cached_only"]}
["原装进口意大利EOS(FORTE)全自动生化分析仪"]
[]
[]
["技术参数"]
["类型","新型的三盘同心结构，任选/批量式全自动生化分析仪"]
["测试方法","终点法、速率法、两点法、双波长法、示差法、双显色剂法、非线性多点定标法（最多可达8点）"]
["测试速度","测试速度：平均360项测试/小时，带电解质最高480项测试/小时（选配）"]
["样品位","118个包括带常规、急诊、质控和标准的样品位"]
["样品量","2—50uL（每0.1uL递增）"]
["样品稀释","自动样品预稀释，并自动对稀释后的样品重测"]
["试剂位","70个试剂位，冷藏系统温度可设在2℃—10℃"]
["试剂量","10—400uL"]
["反应盘","有60个反应杯置于温控孵育池内，孵育池自动混匀"]
["反应总量","100—500uL"]
["反应温度","37℃，±10℃"]
["采样系统","微量特氟龙采样针，带有珀尔贴集成传感器的预热试剂针，精确度为0.1%"]
["光路系统","波长范围：340nm—800nm，有波长自动调零功能，光敏感度0.001A（0—3.00.D范围）"]
["电解质单位","K、Na、CL"]
["质控软件","对于每一个测试定义不同的质控，配有Levey—Jennings质控图、Westgards规则"]
["清洗站","10针比色清洗机，每小时耗水量为：5L，再次使用前自动比色检查"]
["稀释系统","500uL的精密稀释器，按0.1uL递增，误差小于0.5%，并可自动回零"]
["操作系统","管理系统包含质控及统计程序，可显示及打印定标、速率法、终点法的检测曲线。并有批量检测优化及急诊检测设置功能"]
["外置","手触屏、彩色液晶显示器、打印机"]
["环境","工作温度18℃至35℃，相对湿度10到90%"]
["接口","双向RS232接口"]
["体积","（W）70×(D)65×(H)120"]
["上述产品标准配置报价为98万人民币"]
[]
["产品名称",null,"报   价",null,"招  标  价",null,"国家中医局补贴",null,null,"医 院 实 付 金 额"]
["原装意大利进口全自动生化分析仪      EOS—BRAVO FORTE                   ",null,"98万人民币",null,"45万人民币",null,"20万人民币",null,null,"25万人民币"]

{"sheet":"15","index":4,"n_rows":43,"n_cols":10,"rows_kept":43,"merged":[[0,0,0,9],[1,0,1,9],[2,1,2,9],[3,0,18,0],[3,1,3,9],[4,1,4,9],[5,1,5,9],[6,1,6,9],[7,1,7,9],[8,1,8,9],[9,1,9,9],[10,1,10,9],[11,1,11,9],[12,1,12,9],[13,1,13,9],[14,1,14,9],[15,1,15,9],[16,1,16,9],[17,1,17,9],[18,1,18,9],[19,1,19,9],[20,1,20,9],[21,1,21,9],[22,1,22,9],[23,1,23,9],[24,1,24,9],[25,1,25,9],[26,1,26,9],[27,1,27,9],[28,1,28,9],[29,1,29,9],[30,1,30,9],[31,1,31,9],[32,1,32,9],[33,1,33,9],[34,1,34,9],[35,1,35,9],[36,0,38,0],[36,1,36,9],[37,1,37,9],[38,1,38,9],[39,0,39,9],[40,3,40,6],[41,0,41,1],[41,2,41,3],[41,4,41,5],[41,7,41,8],[42,0,42,1],[42,2,42,3],[42,4,42,5],[42,7,42,8]],"flags":["formulas_cached_only"]}
["   ESAOTE"]
["原装进口意大利百胜My LabTM15彩超配置清单"]
[]
["系统基本配置","MyLab 15精巧质优高级主机"]
[null,"CRII高级图像处理技术"]
[null,"超宽频带数字化声束形成器"]
[null,"512-1024数字化通道"]
[null,"170dB动态范围"]
[null,"2D、M型成像"]
[null," 彩色多普勒，脉冲多普勒，动态存档，DVD"]
[null,"彩色能量多普勒"]
[null,"彩色方向能量多普勒"]
[null,"TEI 组织谐波 （心脏、腹部、血管小器官、腔内应用）"]
[null,"电影回放（大于2000帧），M型及多普勒回放"]
[null,"2D、彩色多普勒，脉冲多普勒三同步"]
[null,"多普勒实时自动包络测量"]
[null,"3个标准探头接口"]
[null,"内置一体化图文管理工作站"]
[null,"S-VGA，RGB，S-VHS，复合视频信号输出"]
[null,"标准NTSC/PAL视频"]
[null,"USB存储功能"]
[null,"多种语言操作界面"]
[null,"在线/离线常规测量功能"]
[null,"DICOM 功能"]
[null,"打印和电源系统联线"]
[null,"用户包 (包括操作手册光盘，USB存储驱动器)"]
[null,"外围设备安装指南"]
[null,"模块化 (系统可通过模块升级)"]
[null,"测量分析软件包"]
[null,"OB/Gyn许可 p.n.97154411138 "]
[null,"母婴数据库 p.n.97154 411257"]
[null,"血管应用 p.n.97154 411139"]
[null,"用户自定义测量分析"]
[null,"快速用户自定义设置"]
[null,"彩色打印联线 p.n.97154 402197"]
[null,"15”纯平XVGA显示器"]
["探头标准配置","C5-2 R40超宽频电子凸阵探头"]
[null,"LA523 50mm超宽频电子线阵探头"]
[null,"E8-5 R10 端扫凸阵腔内探头 "]
["上述产品标准配置报价为150万人民币"]
[]
["产品名称",null,"报   价",null,"招 标 价",null,"阳光工程补额度","国家中医局补贴",null,"医院实付金额"]
["原装意大利百胜彩色多普勒超声诊断系统           My LabTM 15           ",null,"150万人民币",null,"59.8万人民币",null,"10万人民币","20万人民币",null,"29.8万人民币"]

{"sheet":"索诺声","index":5,"n_rows":31,"n_cols":11,"rows_kept":31,"merged":[[0,0,0,10],[1,0,1,10],[2,1,2,8],[3,0,3,8],[3,10,30,10],[4,0,4,8],[4,9,30,9],[5,0,5,8],[6,0,6,8],[7,0,7,8],[8,0,8,8],[9,0,9,8],[10,0,10,8],[11,0,11,8],[12,0,12,8],[13,0,13,8],[14,0,14,8],[15,0,15,8],[16,0,16,8],[17,0,17,8],[18,0,18,8],[19,0,19,8],[20,0,20,8],[21,0,21,8],[22,0,22,8],[23,0,23,8],[24,0,24,8],[25,0,25,8],[26,0,26,8],[27,0,27,8],[28,0,28,8],[29,0,29,8],[30,0,30,8]],"flags":["formulas_cached_only"]}
["  SONOSITE"]
["美国原装进口Sonosite 180 plus彩超配置清单及资助价格"]
[]
["         系统基本配置",{"$nulls":8},"招标价","医院实付招标价的25％，  共计6.5万人民币(此项费用为需交纳的税金和运保费)仅限5台"]
["腹部,血管,乳腺,妇科,产科,儿科,心脏,小器官,肌肉骨胳或外科手术.",{"$nulls":8},"26万人民币"]
["5〞高分辨力液晶显示屏，具有亮度和对比度调节"]
["二维灰阶成像"]
["M模式成像"]
["彩色多普勒"]
["脉冲多普勒"]
["连续多普勒"]
["局部放大"]
["二次谐波成像"]
["系统动态范围：接近140dB"]
["帧频：可达100帧/秒"]
["电影回放：可逐帧回放"]
["可内部存储120幅图像，用于脱机打印和回顾"]
["标准NTSC/PAL视频，可连接录像机、视频打印机和外接显示器"]
["常规测量功能：距离卡尺、椭圆法面积、财长测量和容积测量"]
["测量分析软件包：产科标准表格和计算、内置病人检查报告、心脏计算软件"]
["用户界面：用户可通过功能键自定义注释"]
["高：13.3英寸(33.8公分)"]
["宽：7.6英寸(19.8公分)"]
["厚：2.4英寸(6.1公分)"]
["重：含一个探头及电池小于5.4磅(2.4公斤)"]
["交直流两用"]
["电池：可充电式锂电池"]
["交流：采用通用型电源适配器"]
["探头标准配置"]
["C60/5-2MHZ腹部变频探头          一个"]
["C15e/4-2MHZ心脏变频探头         一个"]

{"sheet":"PLDD","index":6,"n_rows":37,"n_cols":8,"rows_kept":37,"merged":[[0,0,1,8],[2,1,2,8],[3,0,8,0],[3,1,3,8],[4,1,4,8],[5,1,5,8],[6,1,6,8],[7,1,7,8],[8,1,8,8],[9,0,12,0],[9,1,9,8],[10,1,10,8],[11,1,11,8],[12,1,12,8],[13,0,18,0],[13,1,13,8],[14,1,14,8],[15,1,15,8],[16,1,16,8],[17,1,17,8],[18,1,18,8],[19,1,19,8],[20,0,25,0],[20,1,20,8],[21,1,21,8],[22,1,22,8],[23,1,23,8],[24,1,24,8],[25,1,25,8],[26,0,32,0],[26,1,26,8],[27,1,27,8],[28,1,28,8],[29,1,29,8],[30,1,30,8],[31,1,31,8],[32,1,32,8],[33,0,33,8],[34,3,34,6],[35,0,35,1],[35,2,35,3],[35,4,35,5],[35,7,35,8],[36,0,36,1],[36,2,36,3],[36,4,36,5],[36,7,36,8]],"flags":["formulas_cached_only"]}
["PLDD经皮激光椎间盘治疗系统简介"]
[]
[]
["治疗原理","利用激光的高能量产生局部生物效应---燃烧、汽化、变性和凝固，"]
[null,"使部分病变椎间盘髓核汽化掉，"]
[null,"以达到减低病变椎间盘的内部压力，"]
[null,"回缩突出的颈、腰椎间盘，解除其对脊髓和/或神经根的压迫，"]
[null,"恢复其正常的生理功能，"]
[null,"消除病人由于椎间盘突出引起的腰腿疼痛、痳木及感觉和/或运动功能障碍的临床症状。"]
["治疗方法","局部麻醉 "]
[null,"在C型臂X光机的监视下，将相应的穿刺针穿至病变椎间盘髓核"]
[null,"拔出穿刺针芯，将光纤沿着穿刺针针管送入至要求的位置"]
[null,"预置激光治疗机的治疗参数，发射激光，使部分髓核汽化，形成空洞，实现椎间盘内的减压"]
["治疗特点","手术时间短：5-10分钟"]
[null,"微创伤口处：1毫米，无疤痕"]
[null,"恢复时间快：术后2小时可下床活动"]
[null,"多间盘治疗：同期可治疗多个椎间盘病变"]
[null,"手术无痛苦：只需局部麻醉，不出血或少出血"]
[null,"安全又可靠：不影响脊柱稳定性、不破坏骨组织，无后遗症和并发症。"]
["治疗范围","颈椎病、颈椎间盘突出症、腰椎间盘突出症"]
["技术指标","激光特质：Nd:YAG(掺钕钇铝石榴石晶体)"]
[null,"输出功率：0.25-15W，可根据临床要求调整"]
[null,"不稳定性：不超过±10%(国际标准±20%)"]
[null,"激光波长：1064nm,可持续汽化，美国PLDD之父Choy教授试验比较后的选择，国际上普遍采用"]
[null,"脉冲频率：5-30Hz,可调"]
[null,"适用电源：200VAC/50Hz"]
["标准配置","主机一套"]
[null,"C型臂一套"]
[null,"工作站一套"]
[null,"床旁监护仪一套"]
[null,"床旁呼吸机一套"]
[null,"骨科手术床一套"]
[null,"防护铅衣二套"]
["上述产品标准配置报价为130万人民币"]
[]
["产品名称",null,"报   价",null,"招 标 价",null,"国家中医局补贴","医院实付金额"]
["PLDD经皮激光椎间盘治疗系统       ",null,"130万人民币",null,"98万人民币",null,"20万人民币","78万人民币"]